skeinforge_application.skeinforge_plugins.craft_plugins.dimension ($Date: 2008/02/05 $) | index /home/enrique/Desktop/backup/babbleold/script/reprap/fabmetheus/skeinforge_application/skeinforge_plugins/craft_plugins/dimension.py

Previous / Next / Contents

`
Dimension adds Adrian's extruder distance E value so firmware does not have to calculate it on it's own and can set the extruder speed in relation to the distance that needs to be extruded. Some printers don't support this. Extruder distance is described at:
http://blog.reprap.org/2009/05/4d-printing.html
and in Erik de Bruijn's conversion script page at:
http://objects.reprap.org/wiki/3D-to-5D-Gcode.php
The dimension manual page is at:
http://fabmetheus.crsndoo.com/wiki/index.php/Skeinforge_Dimension
Nophead wrote an excellent article on how to set the filament parameters:
http://hydraraptor.blogspot.com/2011/03/spot-on-flow-rate.html
Operation
Settings
Extrusion Distance Format Choice
Absolute Extrusion Distance
Relative Extrusion Distance
Extruder Retraction Speed
Filament
Filament Diameter
Filament Packing Density
Retract Within Island
Retraction Distance
Restart Extra Distance
Examples
`

## Operation

The default 'Activate Dimension' checkbox is off. When it is on, the functions described below will work, when it is off, the functions will not be called.

## Settings

### Extrusion Distance Format Choice

Default is 'Absolute Extrusion Distance' because in Adrian's description the distance is absolute. In future, because the relative distances are smaller than the cumulative absolute distances, hopefully the firmware will be able to use relative distance.

#### Absolute Extrusion Distance

When selected, the extrusion distance output will be the total extrusion distance to that gcode line.

#### Relative Extrusion Distance

When selected, the extrusion distance output will be the extrusion distance from the last gcode line.

### Extruder Retraction Speed

Default is 13.3 mm/s.
Defines the extruder retraction feed rate. A high value will allow the retraction operation to complete before much material oozes out. If your extruder can handle it, this value should be much larger than your feed rate.
As an example, I have a feed rate of 48 mm/s and a 'Extruder Retraction Speed' of 150 mm/s.

### Filament

#### Filament Diameter

Default is 2.8 millimeters.
Defines the filament diameter.

#### Filament Packing Density

Default is 0.85. This is for ABS.
Defines the effective filament packing density.
The default value is so low for ABS because ABS is relatively soft and with a pinch wheel extruder the teeth of the pinch dig in farther, so it sees a smaller effective diameter. With a hard plastic like PLA the teeth of the pinch wheel don't dig in as far, so it sees a larger effective diameter, so feeds faster, so for PLA the value should be around 0.97. This is with Wade's hobbed bolt. The effect is less significant with larger pinch wheels.
Overall, you'll have to find the optimal filament packing density by experiment.

### Retract Within Island

Default is off.
When selected, retraction will work even when the next thread is within the same island. If it is not selected, retraction will only work when crossing a boundary.

### Retraction Distance

Default is zero.
Defines the amount the extruder retracts (sucks back) the extruded filament whenever an extruder stop is commanded. Using this seems to help prevent stringing. e.g. If set to 10 the extruder reverses the distance required to pull back 10mm of filament. In fact this does not actually happen but if you set this distance by trial and error you can get to a point where there is very little ooze from the extruder when it stops which is not normally the case.

### Restart Extra Distance

Default is zero.
Defines the restart extra distance when the thread restarts. The restart distance will be the retraction distance plus the restart extra distance.
If this is greater than zero when the extruder starts this distance is added to the retract value giving extra filament. It can be a negative value in which case it is subtracted from the retraction distance. On some Repstrap machines a negative value can stop the build up of plastic that can occur at the start of perimeters.

## Examples

The following examples dimension the file Screw Holder Bottom.stl. The examples are run in a terminal in the folder which contains Screw Holder Bottom.stl and dimension.py.
> python dimension.py
This brings up the dimension dialog.
> python dimension.py Screw Holder Bottom.stl
The dimension tool is parsing the file:
Screw Holder Bottom.stl
..
The dimension tool has created the file:
.. Screw Holder Bottom_dimension.gcode

Previous / Next / Contents

Modules
`` |  |
skeinforge_application.skeinforge_plugins.craft_plugins.__init__ fabmetheus_utilities.archive fabmetheus_utilities.euclidean fabmetheus_utilities.fabmetheus_tools.fabmetheus_interpret | fabmetheus_utilities.gcodec fabmetheus_utilities.intercircle math os | fabmetheus_utilities.settings skeinforge_application.skeinforge_utilities.skeinforge_craft skeinforge_application.skeinforge_utilities.skeinforge_polyfile skeinforge_application.skeinforge_utilities.skeinforge_profile | sys fabmetheus_utilities.geometry.solids.triangle_mesh

Classes
`` |  | DimensionRepository DimensionSkein
class DimensionRepository
`` | `A class to handle the dimension settings.`
| Methods defined here: __init__(self) `Set the default settings, execute title & settings fileName.` execute(self) `Dimension button has been clicked.`
class DimensionSkein
`` | `A class to dimension a skein of extrusions.`
| Methods defined here: __init__(self) `Initialize.` addLinearMoveExtrusionDistanceLine(self, extrusionDistance) `Get the extrusion distance string from the extrusion distance.` getCraftedGcode(self, gcodeText, repository) `Parse gcode text and store the dimension gcode.` getDimensionedArcMovement(self, line, splitLine) `Get a dimensioned arc movement.` getDimensionedLinearMovement(self, line, splitLine) `Get a dimensioned linear movement.` getDistanceToNextThread(self, lineIndex) `Get the travel distance to the next thread.` getExtrusionDistanceString(self, distance, splitLine) `Get the extrusion distance string.` getExtrusionDistanceStringFromExtrusionDistance(self, extrusionDistance) `Get the extrusion distance string from the extrusion distance.` getRetractionRatio(self, lineIndex) `Get the retraction ratio.` getSmallestEnclosureIndex(self, point) `Get the index of the smallest boundary loop which encloses the point.` parseBoundaries(self) `Parse the boundaries and add them to the boundary layers.` parseInitialization(self) `Parse gcode initialization and store the parameters.` parseLine(self, lineIndex) `Parse a gcode line and add it to the dimension skein.`

Functions
`` |  | getCraftedText(fileName, gcodeText='', repository=None) `Dimension a gcode file or text.` getCraftedTextFromText(gcodeText, repository=None) `Dimension a gcode text.` getNewRepository() `Get new repository.` main() `Display the dimension dialog.` writeOutput(fileName, shouldAnalyze=True) `Dimension a gcode file.`

Data
`` |  | __author__ = 'Enrique Perez (perez_enrique@yahoo.com)' __date__ = '$Date: 2008/02/05 $' __license__ = 'GNU Affero General Public License http://www.gnu.org/licenses/agpl.html'

Author
`` |  | Enrique Perez (perez_enrique@yahoo.com)