Cmp-Mod V01 Genere par PcbNew le 20/8/2009-09:15:12

BeginCmp
TimeStamp = 4A86B8B1
Path = /4A86B8B1
Reference = Taladro;
ValeurCmp = 3mm;
IdModule  = Taladro3mm;
EndCmp

BeginCmp
TimeStamp = 4A86DA4C
Path = /4A86DA4C
Reference = CT2;
ValeurCmp = Puerto_B;
IdModule  = CON2X5A;
EndCmp

BeginCmp
TimeStamp = 4A891EAC
Path = 
Reference = Taladro;
ValeurCmp = 3mm;
IdModule  = Taladro3mm;
EndCmp

BeginCmp
TimeStamp = 4A891EB3
Path = 
Reference = Taladro;
ValeurCmp = 3mm;
IdModule  = Taladro3mm;
EndCmp

BeginCmp
TimeStamp = 4A891EB5
Path = 
Reference = Taladro;
ValeurCmp = 3mm;
IdModule  = Taladro3mm;
EndCmp

BeginCmp
TimeStamp = 4A87C300
Path = /4A87C300
Reference = Servo1;
ValeurCmp = Servo1;
IdModule  = CON1X3;
EndCmp

BeginCmp
TimeStamp = 4A87C3EC
Path = /4A87C3EC
Reference = Servo2;
ValeurCmp = Servo2;
IdModule  = CON1X3;
EndCmp

BeginCmp
TimeStamp = 4A87C46E
Path = /4A87C46E
Reference = Servo3;
ValeurCmp = Servo3;
IdModule  = CON1X3;
EndCmp

BeginCmp
TimeStamp = 4A87C492
Path = /4A87C492
Reference = Servo4;
ValeurCmp = Servo4;
IdModule  = CON1X3;
EndCmp

BeginCmp
TimeStamp = 4A87C49F
Path = /4A87C49F
Reference = Servo5;
ValeurCmp = Servo5;
IdModule  = CON1X3;
EndCmp

BeginCmp
TimeStamp = 4A87C4AA
Path = /4A87C4AA
Reference = Servo6;
ValeurCmp = Servo6;
IdModule  = CON1X3;
EndCmp

BeginCmp
TimeStamp = 4A87C4CC
Path = /4A87C4CC
Reference = Servo8;
ValeurCmp = Servo8;
IdModule  = CON1X3;
EndCmp

BeginCmp
TimeStamp = 4A87C4B9
Path = /4A87C4B9
Reference = Servo7;
ValeurCmp = Servo7;
IdModule  = CON1X3;
EndCmp

BeginCmp
TimeStamp = 4A87C592
Path = /4A87C592
Reference = JP5;
ValeurCmp = JP_3;
IdModule  = CON1X3;
EndCmp

BeginCmp
TimeStamp = 4A87DB0F
Path = /4A87DB0F
Reference = S2;
ValeurCmp = RESET;
IdModule  = Pulsador;
EndCmp

BeginCmp
TimeStamp = 4A87B4EE
Path = /4A87B4EE
Reference = S1;
ValeurCmp = PULSADOR;
IdModule  = Pulsador;
EndCmp

BeginCmp
TimeStamp = 4A87B3D3
Path = /4A87B3D3
Reference = JP1;
ValeurCmp = JP_2;
IdModule  = Jumper;
EndCmp

BeginCmp
TimeStamp = 4A86FC39
Path = /4A86FC39
Reference = CT3;
ValeurCmp = Puerto_C;
IdModule  = CON2X5A;
EndCmp

BeginCmp
TimeStamp = 4A881692
Path = /4A881692
Reference = C3;
ValeurCmp = 1uF;
IdModule  = CON-ELE;
EndCmp

BeginCmp
TimeStamp = 4A87ACB6
Path = /4A87ACB6
Reference = T1;
ValeurCmp = ICD2;
IdModule  = RJ11A;
EndCmp

BeginCmp
TimeStamp = 4A86B9C5
Path = /4A86B9C5
Reference = T2;
ValeurCmp = RJ11;
IdModule  = RJ11A;
EndCmp

BeginCmp
TimeStamp = 4A87DBC3
Path = /4A87DBC3
Reference = TRT2;
ValeurCmp = BC547;
IdModule  = TRT-EBC;
EndCmp

BeginCmp
TimeStamp = 4A87A7B7
Path = /4A87A7B7
Reference = TRT1;
ValeurCmp = BC547;
IdModule  = TRT-EBC;
EndCmp

BeginCmp
TimeStamp = 4A86FFFA
Path = /4A86FFFA
Reference = CT4;
ValeurCmp = Puerto_Prog;
IdModule  = CON2x5R;
EndCmp

BeginCmp
TimeStamp = 4A86DA24
Path = /4A86DA24
Reference = CT1;
ValeurCmp = Puerto_A;
IdModule  = CON2X5A;
EndCmp

BeginCmp
TimeStamp = 4A87D0A2
Path = /4A87D0A2
Reference = JP7;
ValeurCmp = JP_2;
IdModule  = Jumper;
EndCmp

BeginCmp
TimeStamp = 4A87CFA4
Path = /4A87CFA4
Reference = JP6;
ValeurCmp = JP_2;
IdModule  = Jumper;
EndCmp

BeginCmp
TimeStamp = 4A87CFE8
Path = /4A87CFE8
Reference = R8;
ValeurCmp = 4K7;
IdModule  = RES14W;
EndCmp

BeginCmp
TimeStamp = 4A87D086
Path = /4A87D086
Reference = R7;
ValeurCmp = 4K7;
IdModule  = RES14W;
EndCmp

BeginCmp
TimeStamp = 4A87B6C5
Path = /4A87B6C5
Reference = D1;
ValeurCmp = LED;
IdModule  = LED3mm;
EndCmp

BeginCmp
TimeStamp = 4A87B665
Path = /4A87B665
Reference = JP2;
ValeurCmp = JP_2;
IdModule  = Jumper;
EndCmp

BeginCmp
TimeStamp = 4A87B6DA
Path = /4A87B6DA
Reference = R5;
ValeurCmp = 330;
IdModule  = RES14W;
EndCmp

BeginCmp
TimeStamp = 4A86D882
Path = /4A86D882
Reference = U1;
ValeurCmp = PIC16F876A;
IdModule  = DIL28-3;
EndCmp

BeginCmp
TimeStamp = 4A86C99A
Path = /4A86C99A
Reference = U2;
ValeurCmp = MAX232;
IdModule  = DIL16-3;
EndCmp

BeginCmp
TimeStamp = 4A8816AF
Path = /4A8816AF
Reference = C4;
ValeurCmp = 100nF;
IdModule  = CON-MUL;
EndCmp

BeginCmp
TimeStamp = 4A86B8B1
Path = /4A86B8B1
Reference = C5;
ValeurCmp = 1uF;
IdModule  = CON-ELE;
EndCmp

BeginCmp
TimeStamp = 4A86D225
Path = /4A86D225
Reference = C6;
ValeurCmp = 1uF;
IdModule  = CON-ELE;
EndCmp

BeginCmp
TimeStamp = 4A86CD35
Path = /4A86CD35
Reference = C7;
ValeurCmp = 1uF;
IdModule  = CON-ELE;
EndCmp

BeginCmp
TimeStamp = 4A86D243
Path = /4A86D243
Reference = C8;
ValeurCmp = 1uF;
IdModule  = CON-ELE;
EndCmp

BeginCmp
TimeStamp = 4A87DC20
Path = /4A87DC20
Reference = JP4;
ValeurCmp = JP_3;
IdModule  = CON1X3;
EndCmp

BeginCmp
TimeStamp = 4A87D75D
Path = /4A87D75D
Reference = JP3;
ValeurCmp = JP_3;
IdModule  = CON1X3;
EndCmp

BeginCmp
TimeStamp = 4A87D9B4
Path = /4A87D9B4
Reference = C1;
ValeurCmp = 22pF;
IdModule  = CON-MUL;
EndCmp

BeginCmp
TimeStamp = 4A87D9F6
Path = /4A87D9F6
Reference = C2;
ValeurCmp = 22pF;
IdModule  = CON-MUL;
EndCmp

BeginCmp
TimeStamp = 4A87D994
Path = /4A87D994
Reference = X1;
ValeurCmp = 20MHZ;
IdModule  = XTAL-R;
EndCmp

BeginCmp
TimeStamp = 4A87D744
Path = /4A87D744
Reference = R1;
ValeurCmp = 10K;
IdModule  = RES14W;
EndCmp

BeginCmp
TimeStamp = 4A87B476
Path = /4A87B476
Reference = R6;
ValeurCmp = 4K7;
IdModule  = RES14W;
EndCmp

BeginCmp
TimeStamp = 4A870E05
Path = /4A870E05
Reference = R3;
ValeurCmp = 4K7;
IdModule  = RES14W;
EndCmp

BeginCmp
TimeStamp = 4A87DBE4
Path = /4A87DBE4
Reference = R4;
ValeurCmp = 10K;
IdModule  = RES14W;
EndCmp

BeginCmp
TimeStamp = 4A87A725
Path = /4A87A725
Reference = R2;
ValeurCmp = 10K;
IdModule  = RES14W;
EndCmp

BeginCmp
TimeStamp = 4A87CF25
Path = /4A87CF25
Reference = CT5;
ValeurCmp = I2C;
IdModule  = CON1X4;
EndCmp

BeginCmp
TimeStamp = 4A881D19
Path = /4A881D19
Reference = CT6;
ValeurCmp = JP_5;
IdModule  = CON1X5;
EndCmp

BeginCmp
TimeStamp = 4A87C6E7
Path = /4A87C6E7
Reference = CL2;
ValeurCmp = Vext;
IdModule  = CLEMA-2V;
EndCmp

BeginCmp
TimeStamp = 4A88126A
Path = /4A88126A
Reference = CL1;
ValeurCmp = Power;
IdModule  = CLEMA-2V;
EndCmp

BeginCmp
TimeStamp = 4A881250
Path = /4A881250
Reference = J1;
ValeurCmp = JACK;
IdModule  = Jack;
EndCmp

EndListe
