fabmetheus_utilities.fabmetheus_tools.interpret_plugins.slc ($Date: 2008/21/04 $) | index /home/enrique/Desktop/backup/babbleold/script/reprap/fabmetheus/fabmetheus_utilities/fabmetheus_tools/interpret_plugins/slc.py

Previous / Next / Contents

`
The slc.py script is an import translator plugin to get a carving from an slc file.
An import plugin is a script in the interpret_plugins folder which has the function getCarving. It is meant to be run from the interpret tool. To ensure that the plugin works on platforms which do not handle file capitalization properly, give the plugin a lower case name.
The getCarving function takes the file name of an slc file and returns the carving.
An explanation of the SLC format can be found at:
http://rapid.lpt.fi/archives/rp-ml-1999/0713.html`

Previous / Next / Contents

Modules
`` |  |
__init__ fabmetheus_utilities.euclidean | fabmetheus_utilities.gcodec math | fabmetheus_utilities.svg_writer sys |

Classes
`` |  | SLCCarving SampleTableEntry
class SLCCarving
`` | `An slc carving.`
| Methods defined here: __init__(self) `Add empty lists.` __repr__(self) `Get the string representation of this carving.` addXML(self, depth, output) `Add xml for this object.` getCarveCornerMaximum(self) `Get the corner maximum of the vertexes.` getCarveCornerMinimum(self) `Get the corner minimum of the vertexes.` getCarveLayerThickness(self) `Get the layer thickness.` getCarveRotatedBoundaryLayers(self) `Get the rotated boundary layers.` getCarvedSVG(self) `Get the carved svg text.` getFabmetheusXML(self) `Return the fabmetheus XML.` getInterpretationSuffix(self) `Return the suffix for a carving.` processContourLayers(self, file) `Process a contour layer at a time until the top of the part.` readFile(self, fileName) `Read SLC and store the layers.` readTableEntry(self, file) `Read in the sampling table section. It contains a table length (byte) and the table entries.` setCarveImportRadius(self, importRadius) `Set the import radius.` setCarveInfillInDirectionOfBridge(self, infillInDirectionOfBridge) `Set the infill in direction of bridge.` setCarveIsCorrectMesh(self, isCorrectMesh) `Set the is correct mesh flag.` setCarveLayerThickness(self, layerThickness) `Set the layer thickness.`
class SampleTableEntry
`` | `Sample table entry.`
| Methods defined here: __init__(self, file) `Read in the sampling table section. It contains a table length (byte) and the table entries.` __repr__(self) `Get the string representation of this sample table entry.`

Functions
`` |  | getCarving(fileName='') `Get the triangle mesh for the slc file.` getLittleEndianFloatGivenFile(file) `Get little endian float given a file.` getLittleEndianUnsignedLongGivenFile(file) `Get little endian float given a file.` getPointsFromFile(numPoints, file) `Process the vertice points for a given boundary.` main() `Display the inset dialog.` readHeader(file) `Read the slc header.`

Data
`` |  | __author__ = 'Enrique Perez (perez_enrique@yahoo.com)' __credits__ = 'Nophead <http://hydraraptor.blogspot.com/>\nArt of Illusion <http://www.artofillusion.org/>' __date__ = '$Date: 2008/21/04 $' __license__ = 'GNU Affero General Public License http://www.gnu.org/licenses/agpl.html' absolute_import = _Feature((2, 5, 0, 'alpha', 1), (2, 7, 0, 'alpha', 0), 16384)

Author
`` |  | Enrique Perez (perez_enrique@yahoo.com)

Credits
`` |  | Nophead <http://hydraraptor.blogspot.com/> Art of Illusion <http://www.artofillusion.org/>